 Green Life Group

TECHNICAL DATA SHEET

 GREEN UP FORTE

Description

A Safe cleaner and sterilizer powerful, biodegradable, water based degreaser,

oil dispersant and sanitizer. GREEN UP FORTE is a powerful non chlorinated cleaner for the cleaning of metallic surfaces special for heat transfer systems. Does not damage rubber, plastic, metal or stainless steel surfaces  
 GREEN UP FORTE is a water based degreaser and oil dispersant, which has proved to be a versatile cleaning agent in factory and workshop situations where degreasing cleaning or where a fast drying solvent cleaner is required.  
GREEN UP FORTE is made from renewable raw materials –glucose derived from corn, and  fatty alcohols from coconut and palm kernel oils due to its natural chemistry, mixt with natural silicates.  This product is very mild, low in toxicity and readily Biodegradable      

Applications

* Engine cleaning
* Lorry chassis cleaning
* Sewers and sewage pipes Machinery cleaning
* Garage floor cleaning
* Garage pit cleaning
* Factory floor and wall cleaning
* Oilrig cleaning
* Final stage clean up of oil pollution and oil spills
* Printing Industry cleaning
* Food industry Including kitchens and dining rooms
* Electric Motors
* Air Conditioning system

Green Life Group

TECHNICAL DATA SHEET

 GREEN UP FORTE

-2-

Summary of Benefits

Food Save  
Water based degreaser  
Can be diluted with water  
Can be applied in wet areas  
Free from Chlorinated Solvents  
Not harm the Environment  Cleaner and sterilizer combined    
Nonflammable  
Does not  discharge toxic gas or synthetic solvent smell   
Does not risk the breathing way    
Does not attacking  the surface, not damage plastic, rubber and metals.

Methods

 To remove heavy soiling, apply neat with brush or sprayer, leave for 5 to 10 minutes then rinse off with water.

Where soiling is not too heavy,

GREEN UP FORTE can be diluted with water before application.  
GREEN UP FORTE can be used through floor scrubbing machines; the dilution rate would need to be established

By trial and error, as all machines are different.  
GREEN UP FORTE can also be used by simply diluting a small amount with water in a bucket; the affected area is then

Cleaned with a brush or mop, before rinsing.  This method is ideal on lightly soiled floors in canteens, toilets and shower areas.  
 In the case of large oil spills, clear away as much as possible, then use GREEN UP FORTE (neat) in the final clean up stage.

Green Life Group

TECHNICAL DATA SHEET

 GREEN UP FORTE

-3-

 Direction for Use   
General Cleaning   
To clean fat friers, cooker hoods, etc. Use at 1:2 dilution with water, apply by mop, brush, or spray onto the surface, allow to soak, then rinse off using water.  
To clean heavily contaminated areas dilute at 1:2 with water and apply, allow to soak then wash off with clean water.  
To clean general areas including floors etc. dilute at 1:3 with water apply using a mop, brush, or spray, allow to soak then rinse. If used as a hand cleaner then the product must be diluted to at least 1:3 with water.  
For the cleaning of air-conditioning units use at 1:3 with water  
The product is also suitable for use in automatic foam spray units.  
   
 For Heat Exchanger Cleaning

Isolate the oil supply, disconnect the heat exchanger oil inlet and outlet, drain off any remaining oil.

Connect the discharge side of Cleaning Unit (CU) to the lower heat exchanger connection and fit the return to the CU.

Add HEC to the drum and heat, maintaining the temperature (max 65°C) throughout the cleaning operation FOR 8-10 hours.

If heating is not available, and fit the return to the CU Circulate for 24 hours. When the cleaning is complete, disconnect the lower heat exchanger connection and drain.

Connect a high pressure fresh water supply to the upper heat exchanger connection. Rinse until water runs clear.

Disconnect, drain and dry.

PHYSICAL PROPERTIES

Colour: - Pale Colored

Odour - Barely perceptible odour

Density                                   -           1.06  
Flash Point                             -           None

Flammability: - None Flammable

Boiling Temperature/ range - >100 C

Solubility in water                   -           Immiscible

Green Life Group

TECHNICAL DATA SHEET

 GREEN UP FORTE

-4-

Components

 NATURAL non caustic readily biodegradable water based components

 None of the components is made of neither animals.  
 The liquid does not contains minerals fats, or fats produce from animals  
 Green Life Group is against experiments in animals and does not include    
 in its products components from them.

Health and safety

For full Health and Safety data please refer to our specific MSDS Sheet, which is available on Product list.  
   
Pack Sizes

4lt, 18lt , 205lt barrels, 1000 litter canister 

Shelf Life

 3 Years from date of manufacture